{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"defined_names":2},"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":22,"n_cols":11,"rows_kept":22,"merged":[[1,0,1,10],[21,1,21,10]]}
["附件"]
["2022年电器附件产品质量国家监督抽查不合格产品　　\n　　　及企业名单"]
["序号","产品种类","受检单位","标称生产单位","标称生产单位所在地","产品名称","规格型号","生产日期/批号","主要不合格项目","承检机构","备注"]
[1,"家用和类似用途固定式电气装置的开关（墙壁开关）","温州锐客科技有限公司","温州锐客科技有限公司","浙江省","暗装跷板式单极开关","1K1 10AX 250V～",2022.07,"耐热*","威凯检测技术有限公司"]
[2,"隔离开关","三信国际电器上海有限公司","三信国际电器上海有限公司","上海市","隔离开关","3SG6","2022年6月/2022/6","短路性能能力*","浙江省机电产品质量检测所有限公司"]
[3,"隔离开关","江苏省中仁电气有限公司","江苏省中仁电气有限公司","江苏省","隔离开关","SZRG2-125/1 32A","2022年8月/2022-08","短路性能能力*","浙江省机电产品质量检测所有限公司"]
[4,"隔离开关","浙江斯维奇物联技术有限公司","浙江斯维奇物联技术有限公司","浙江省","负荷隔离开关","NWGL-160","2022-08/2022-08","短路性能能力*","浙江省机电产品质量检测所有限公司"]
[5,"隔离开关","朗明电气有限公司","朗明电气有限公司","浙江省","负荷隔离开关","SGL-250/3P","2022-03/2022-03","接通和分断能力*","浙江省机电产品质量检测所有限公司"]
[6,"隔离开关","浙江海机所电气有限公司","浙江海机所电气有限公司","浙江省","隔离开关","HJDG7-125","2022年6月/2022年6月","短路性能能力*","浙江省机电产品质量检测所有限公司"]
[7,"隔离开关","浙江梦融电力科技有限公司","浙江梦融电力科技有限公司","浙江省","隔离开关","MRHL（MRG1）-125","2022-7/6","短路性能能力*","浙江省机电产品质量检测所有限公司"]
[8,"隔离开关","浙江双通电气有限公司","浙江双通电气有限公司","浙江省","隔离开关","STHGL-160/3","2022-06/2022-06","短路性能能力*","浙江省机电产品质量检测所有限公司"]
[9,"隔离开关","乐清市永信熔断器厂","乐清市永信熔断器厂","浙江省","隔离开关","HY122-63","2022-08-19/2022-08","短路性能能力*","浙江省机电产品质量检测所有限公司"]
[10,"隔离开关","浙江全启电气科技有限公司","浙江全启电气科技有限公司","浙江省","隔离开关","ZQG-125 32A","2022年8月/2022-08","短路性能能力*","浙江省机电产品质量检测所有限公司"]
[11,"隔离开关","浙江约拿电气有限公司","浙江约拿电气有限公司","浙江省","隔离开关","MKG1（MG1）-100B","2022-06-20/2022-06","短路性能能力*","浙江省机电产品质量检测所有限公司"]
[12,"隔离开关","洛普电气有限公司","洛普电气有限公司","浙江省","负荷隔离开关","HGL（GL）-32/3","2022-08/2022-08","短路性能能力*","浙江省机电产品质量检测所有限公司"]
[13,"延长线插座（带电源适配器）","浙江创奥电器有限公司","浙江创奥电器有限公司","浙江省","延长线插座（带电源适配器）","C1-W305U 10A 250V～ MAX 2500W USB模块输入：220V～,50Hz,350mA USB模块输出：5VDC 2.1A MAX","2022年5月/DT.22.05","防触电保护*","初检机构：威凯检测技术有限公司\n复检机构：广东产品质量监督检验研究院(国家电器产品安全质量监督检验中心)","复检仍不合格"]
[14,"延长线插座（带电源适配器）","临海市绿导电器有限公司","临海市绿导电器有限公司","浙江省","延长线插座（带电源适配器）","LD017/1P4U 10A 250V ～ MAX2500W （配60227 IEC53 3×1mm²）HGL（GL）-32/3\nUSB 输入:220-250V～,\n50/60Hz,0.5A;单口最大输出：\n5V MAX2.4A,USB 总输出：\n5V MAX2.4A(仅适用于海拔2000米及以下)","2022/9/6","延长线插座的结构*,电气间隙、爬电距离*","威凯检测技术有限公司"]
[15,"延长线插座（带电源适配器）","森森集团股份有限公司","森森集团股份有限公司","浙江省","延长线插座（带电源适配器）","AQ-600 MAX 2500W MAX 10A 250V～（配线 60227IEC53 3×1mm²）;USB 额定输入：\n220V～,50Hz 0.2A；USB 模块输\n出：5VDC 0.2A（仅适用于海拔\n2000 米及以下；仅适用于非热带气候条件）","2021/4/1","防触电保护*,耐热*","初检机构：威凯检测技术有限公司\n复检机构：广东产品质量监督检验研究院(国家电器产品安全质量监督检验中心)","复检仍不合格"]
[16,"延长线插座（带电源适配器）","浙江捷诺电器股份有限公司","浙江捷诺电器股份有限公司","浙江省","延长线插座（带电源适配器）","C1-W305U 插座：10A 250V～ MAX 2500W USB模块输入：220V～,50Hz,350mA USB模块输出：5VDC 2.1A MAX","2022年5月17日/DT.22.05","防触电保护*","初检机构：威凯检测技术有限公司\n复检机构：广东产品质量监督检验研究院(国家电器产品安全质量监督检验中心)","复检仍不合格"]
[17,"延长线插座（带电源适配器）","浙江创奥电器有限公司","浙江来风工具有限公司","浙江省","延长线插座（带电源适配器）","C1-W305U ：MAX 10A 250V～ MAX 2500W USB模块输入：220V～,50Hz,350mA USB模块输出：5VDC 2.1A MAX","2022年5月/DT.22.05","防触电保护*","初检机构：威凯检测技术有限公司\n复检机构：广东产品质量监督检验研究院(国家电器产品安全质量监督检验中心)","复检仍不合格"]
[18,"延长线插座（带电源适配器）","深圳市极质科技有限公司","深圳市极质科技有限公司","广东省","延长线插座（带电源适配器，智能插线板）","JZZNCXB00 插座：2500W MAX 10A MAX 250V～（配60227 IEC53 3×1mm² ）;USB 额定输入：\n100-240V～,50/60Hz,0.5A;\nUSB 单口输出：5VDC 2A，9VDC \n2A，12VDC 1.5A；USB 总输出：\n5VDC 3.6A 18W MAX （仅适用于海拔 2000 米及以下地区使用）","2022/3/24","耐热*","威凯检测技术有限公司"]
[null,"注： 1.按产品及行政区域排序。\n         2.复检仍不合格，指产品初检不合格，企业提出复检申请，经复检产品仍不合格。\n         3.加*号的项目为安全项目。"]